Sidewinder 8220

ROLLER BLIND SYSTEM WITH CHAIN OPERATION

Suitable for installation on a frame in domestic or professional environments.   
150 cm W max. - 250 cm H max.; weight not greater than 1.5 kg with filtering, dimming or reflecting fabrics.  
Ceiling or wall installation.   
Aluminium winding tube and base.  
Direct clutch with chain operation.  
Thermoplastic brackets with 30 mm and 42 mm projection.